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 *************************************************************************************************************************
ÖFFENTLICHE AUSSCHREIBUNG / PUBLIC ANNOUNCEMENT

Floor replacement project at commercial kitchen


**************************************************************************************************************************

The U.S. Consulate General Frankfurt invites you to submit offers for a firm fixed price for:
Das US Konsulat Frankfurt bittet Sie ein Pauschalangebot für die folgenden Leistungen zu übermitteln:




1.	Conditions

The contractor is advised that–

•	Normal US Consulate working hours are 08:00-16:30hrs Monday – Friday.
[bookmark: _GoBack]•	The Principle Contractor who is awarded the project/contract shall be named within this document as the contractor. 
•	The contractor shall familiarize him/herself fully with this specification document and include for all materials, labor and equipment costs to complete the tasks and actions that are specified within this document.
•	The Consulate operates strict security procedures for entry into the building, all tradesmen’s/women’s details shall be provided to the Contracting Officers Representative (COR) a minimum 48 hours before visiting building. 
•	All of his/her employees shall require security clearance before being allowed to work at the Consulate or Government owned/long term leased properties; to obtain clearance each employee shall complete all required security clearance forms. 
•	When working within residential buildings the contractor shall ensure that all doors remain closed/locked at all times and ensure the properties are left secure at the end of each working day.
•	Security at the residential properties shall be the contractor’s responsibility throughout the duration of the project.
•	Access to the property is limited and only with agreement by either the occupant or the COR.
•	No work shall be started or materials ordered until the contractor has received a purchase order for the works or has been given notice by the Contracting Officer.
•	The costs of additional work performed by the contractor not described in this specification and not approved in writing by the U.S. Government shall be borne by the contractor.
•	No work shall be completed on American/German holidays unless by prior arrange/agreement and at no addition costs to the US Government.
•	The contractor is responsible for all site management including all Health & Safety, welfare & first aid facilities, employment/managing/programming of sub-contractors and site security. 
•	The contractor shall provide the Contracting Officers Representative (COR) with all risk assessments and method statements prior to starting on site.
•	The contractor shall provide the COR a detailed program of works mapping each major task, from project start to completion finish.
•	It’s the contractor’s responsibility to ensure that all project tasks specified within the specification/drawings adhere to all HSE guidelines. 
•	Visually display, all health and safety documents and copy of public liability insurance and project specification/drawings. 
•	Where the Contractor considers that the execution of any Order for work will, or is likely to, involve any interference with asbestos-based materials, lead, gas piping or storage containers, pipes conveying steam and any other hazardous substances or installations, he shall immediately stop work and forthwith notify the COR who will give the Contractor further instructions.
•	The contractor shall request a hot works permit prior to starting any soldering/welding work.
•	The contractor shall provide competent a foreman or leading hand on site whilst the project is in progress and he/she shall keep a copy of the specification, visitor log, and necessary Health & Safety logs daily updated, ready for inspection at any time by the “Contracting Officers Representative”.
•	Only competent skilled tradesmen shall be employed to execute all aspects of the works.
•	All work must be executed strictly in accordance with the current Codes of Practice.
•	The contractor shall provide a complete Health & Safety/Operations file for completed works, including all operating instructions and service manuals for all appliances, equipment and materials installed, with details of all guarantees. Include all project COSH data sheets for materials within this document.
•	Complete recycle program for all materials that are to be karted away.
•	All works to be completed in accordance with relevant German/American Standards.
•	The contractor is responsible for their own tools at all times and shall provide a lockable tool/material box for their operative’s tools and materials if/when required.
•	Portables radios or other portable music devices are only allowed at residential buildings if the volume is low and shall not cause any nuisance to neighboring occupants and residents.
•	No Smoking on premises. 


2.	Background

Facilities Management planned the replacement of the existing kitchen floor covering with resin-bonded floor covering to comply with regulations for industrial kitchens.
Furnish all labor, tools, equipment, and materials to install a resin-bonded flooring system in existing kitchen. Prepare existing floors for the installation of the new flooring system in accordance with the manufacturer’s recommendations. Install the new flooring system in accordance with the manufacturer’s recommended installation process and specifications.
Clean all work areas and remove all trash, debris, etc. from premises.
Approximate work area is 98 square meter. There will be a pre-bid meeting during which all work areas will be visited and will allow contractors to get final measurements.
The contractor shall ensure that they familiarize themselves with the technical specification prior to the arranged site visit.
From notice to proceed the contractor has 20 calendar days to complete the project.
 

The contractor shall keep a clean site and ensure tools & materials stowed in a safe manner.


3.	Description

Facilities Management planned the replacement of the existing kitchen floor covering with resin-bonded floor covering to comply with regulations for industrial kitchens at the COB, Bldg.338. That includes delivery of all needed material and installation.  


4.	General Requirements/Equipment

Successful bidder shall, be approved by the manufacturer to install the specified flooring system.
Store all materials in locations approved by the Owner.
Keep work areas neat and clean.
Take all necessary measures to ensure worker and occupant safety. 

UNTERGRUNDVORBEHANDLUNG – Base Surface Preparation
Vorhandene Bodenfläche mit Diamantschleifmaschine abschleifen
Grind existing floor surface with a diamond grinder
98 square meter

Vorhandene Bodenfläche mit Industriestaubsauger feinreinigen
Fine clean existing floor surface with industrial vacuum cleaner
98 square meter 

Einschneiden von Begrenzungs-, Verankerungsschnitten mit Diamantsäge
Cutting boundary, anchoring cuts with diamond saw
7,50 lfdm/running meter

BODENBESCHICHTUNGSARBEITEN
Bodenfläche wie Beton und Zementestriche mit Silikal R51/R52 grundieren  
Prime floor surface such as concrete and cement screeds with Silikal R51/R52
98 square meter

Kratzspachtelung Silikal RV368 zum Ausgleich leichter Bodenunebenheiten, zum schliessen von Betonlunkern und als Grundbeschichtung 
Scratch filler Silikal RV368 to compensate for slight unevenness in the floor, to close concrete voids and as a base coat
98 square meter

Beschichtung Silikal R62 CQ, Schichtdicke ca. 3-4 mm, Farbton entsprechend der Coloritquarzkarte
Coating Silikal R62 CQ, layer thickness approx. 3-4 mm, color according to the colorit quartz map
98,00 qm

Rutschfeste Oberfläche der Beschichtungssysteme durch Abstreuung mit Coloritquarzsanden entsprechender Korngrößen
Non-slip surface of the coating systems by means of dispersion with colorant quartz sands of corresponding particle sizes
90 qm

Deckversiegelung Silikal R71e/R72/R81
Cover seal Silikal R71e/R72/R81
98 qm

Einbringung einer Hohlkehle als Flaschenhohlkehle bzw, Dreickskehle als Zulage
Incorporation of a groove or triangular throat as a supplement
80 lfdm/running meter

Anarbeiten der Beschichtungssysteme bestehenden Bodenbelägen, Rinnen, Tueren, Abläufe usw.
Working the coating systems on existing floor coverings, gutters, doors, drains
7,50 lfdm/running meter

Einbau von Abschlußschienen entsprechend der Beschichtungsstärke
Fabrikat Schlüter, Typ Edelstahl
Installation of end rails according to the coating thickness
     Manufacturer Schlüter, type stainless steel
25,00 lfdm/running meter













Regiearbeiten

Für anfallende Regiearbeiten, die nicht nach qm, lfm oder Stk. Angeboten werden können, wie zB. Aufschneiden und schließen von Rissen, Egalisieren von Ausbrüchen, Korrigieren von falschem Gefälle, Egalisieren von Unebenheiten, Ersetzen von ausgebrochenem Beton-bzw. Estrichuntergründen mit Kunstharzmörtel, Trocknen von nassen Untergründen usw.
For unforeseen work which can’t be offered to square meter, running meter or pieces such as cutting and closing cracks, equalizing outbreaks, correcting false slopes, leveling unevenness, replacing broken concrete or concrete. Screed substrates with resin-based mortar, drying of wet surfaces, etc.
	
4 Monteurstunden / Labor costs			
6 Silikal R51, R52, RU727
300 KG. Kunstharzmörtel/ resin-based mortar R17


Baustelleneinrichtung
	 
An- und Abtransport der Materialien, Vorhalten der erforderlichen Geräte und Maschinen, An- und Abreise der Montagekolonne
Supply and removal of materials, provision of necessary equipment and machinery, arrival and departure of the assembly crew
5.	Safety

Contractor and contractor employees must adhere to all US Construction safety including the following:

	Have a dedicated safety coordinator on site at all times.
	Conduct weekly safety meeting and record minutes and submit minutes to COR
	All workers must wear US required Personal Protection Equipment (PPE) including :
o	Hard hats
o	Googles/safety glasses
o	Safety Shoes
o	Hearing protection
o	Protective gloves
o	Dust masks
o	Respirators
	Construction safety plan 
	Crane operations plan
	Provide all material safety data sheets and insure copies are available at project site.

6.	Quality

Once installed, all products shall be checked if fully operational. An approved quality checklist shall be given to the COR after installation. The Government will not be liable for any breakages or damages to materials whilst they are on site and will only accept products once project is completed and snagging completed.


7.	 Installation

Ensure that floor coverings/finishes and surrounding areas are protected are protect against damages.
Take measures to stop the spread of dust through the house.


8.	Completion

The contractor shall conduct on site quality checks prior to project completion/acceptance and advise Facility Management Office when product is ready for snagging.
Remove all unused materials and equipment from site. 


9.	Future Maintenance

Provide detailing periodic maintenance requirements.


10.	Personnel Security

The US Government reserves the right to deny access to U.S.-owned and operated facilities to any individual.  The Contractor shall provide the needed Security Information’s on all personnel provided for this contract prior to their utilization.  All of his/her employees shall require security clearance before being allowed to work at the Consulate or Government owned/long term leased properties; to obtain clearance each employee shall complete all required security clearance forms. 
Submission of information shall be made within 10 days of award of contract. No technician will be allowed on site without prior authorization. Note: this may include cleared personnel if advance notice of visit is not given at least one week before the scheduled arrival.






Site visit:
Besichtigungstermin:
7 September , 2018 (bitte unbedingt mindestens 48 Stunden im Voraus anmelden) 

Shipping terms:
Lieferbedingungen:
Including delivery to the Consulate General Frankfurt.
Inklusive Lieferung an das örtliche Generalkonsulat in Frankfurt

Payment terms:
Zahlungsbedingungen:
Payment terms are to be 30 days after Government acceptance of supplies delivered/
Rechnungsstellung nach Lieferung mit 30 Tagen Zahlungsziel

Request for Quotation Number:
Ausschreibungsnummer:
PR7634830

Due date for quotation: 
Letzter Abgabetermin:
18 September, 2018	

The responsible purchasing agent for this announcement would be:
Der zuständige Ansprechpartner für diese Ausschreibung ist:


Purchasing Agent:  Thomas Petersen
E-Mail: FrankfurtGSOProcurementTeam@state.gov
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